Life-saving appliances packed in strong rigid outer packagings with a total maximum gross mass not exceeding 40 kg, containing no dangerous goods other than Division 2.2 compressed or liquefied gases (with no subsidiary hazard) contained in receptacles with a capacity not exceeding 120 mL and installed solely for the purpose of the activation of the appliance, are not subject to these Instructions when carried as cargo.