Combination packagings are allowed.

Part 4, Chapter 1 requirements must be met, including:

1) Compatibility requirements

- Substances must be compatible with their packagings as required by 4;1.1.3.

- Metal packagings must be corrosion resistant or be protected against corrosion for substances with a Class 8 subsidiary hazard.

2) Closure requirements

- Closures must meet the requirements of 4;1.1.4.

Cylinders as permitted by 4;2.7 are allowed.

Packagings must meet the Packing Group II performance requirements if the substance has a Class 8 subsidiary hazard.

----------
For this substance the special provision A9 of table 3-1 can apply:

Special provision A9:
Alcoholic beverages containing not more than 70 per cent alcohol by volume, when packed in receptacles of 5 litres or less, are not subject to these Instructions when carried as cargo.