Verpackungsanweisung 964 (für UN 3151)

Passenger and cargo aircraft for UN 3151 only

General requirements

Part 4, Chapter 1 requirements must be met. These requirements include:

1) Compatibility requirements

- Substances must be compatible with their packagings as required by 4;1.1.3.

2) Closure requirements

- Closures must meet the requirements of 4;1.1.4.

------------------------------------------------------------------
                       COMBINATION PACKAGINGS 
------------------------------------------------------------------
                         |         |Inner      |Total    |Total
                         |  Inner  |packaging  |quantity |quantity
                         |packaging|quantity   |  per    |  per
UN number and proper     |  (see   | (per      |package -|package-
shipping name            |  6;3.2) |receptacle)|passenger| cargo
------------------------------------------------------------------
UN 3151 Polyhalogenated  |  Glass  |  10.0 L   |         |
   biphenyls, liquid or  |---------------------|         |
   Polyhalogenated       | Plastics|  30.0 L   |         |
   terphenyls, liquid or |         |           |  100 L  | 220 L
   Halogenated mono-     |---------------------|         |
   methyldiphenyl-       |  Metal  |  40.0 L   |         |
   methanes,liquid|      |         |           |         |
------------------------------------------------------------------

OUTER PACKAGINGS OF COMBINATION PACKAGINGS (see 6;3.1)

Boxes                        Drums                     Jerricans

Aluminium (4B)               Aluminium (1B1, 1B2)      Aluminium (3B1, 3B2)
Fibreboard (4G)              Fibre (1G)                Plastics (3H1, 3H2)
Natural wood (4C1, 4C2)      Other metal (1N1, 1N2)    Steel (3A1, 3A2)
Other metal (4N)             Plastics (1H1, 1H2)            
Plastics (4H1, 4H2)          Steel (1A1, 1A2)
Plywood (4D)
Reconstituted wood (4F)
Steel (4A)