N_LFDNR	S_UNCODIERUNG	S_TEXT	S_SPRACHE
0		General packing requirements	E
1	11A	Rigid steel IBC for solids, filled or discharged by gravity	E
2	11B	Rigid aluminium IBC for solids, filled or discharged by gravity	E
3	11N	Rigid metal (other than steel or aluminium) IBC for solids, filled or discharged by gravity	E
4	11G	Rigid fibreboard IBC for solids, filled or discharged by gravity	E
5	11C	Rigid natural wood IBC for solids, filled or discharged by gravity	E
6	11D	Rigid plywood IBC for solids, filled or discharged by gravity	E
7	11F	Rigid reconstituted wood IBC for solids, filled or discharged by gravity	E
8	11H1	Rigid plastics IBC for solids, with structural equipment, filled or discharged by gravity	E
9	11H2	Rigid plastics IBC for solids, freestanding, filled or discharged by gravity	E
10	11HA1	Composite IBC with a rigid plastics inner receptacle encased in a rigid steel outer casing, for solids filled or discharged by gravity	E
11	11HH1	Composite IBC with a rigid plastics inner receptacle encased in a rigid plastics outer casing, for solids filled or discharged by gravity	E
12	11HB1	Composite IBC with a rigid plastics inner receptacle encased in a rigid aluminium outer casing, for solids filled or discharged by gravity	E
13	11HC1	Composite IBC with a rigid plastics inner receptacle encased in a rigid natural wood outer casing, for solids filled or discharged by gravity	E
14	11HD1	Composite IBC with a rigid plastics inner receptacle encased in a rigid plywood outer casing, for solids filled or discharged by gravity	E
15	11HF1	Composite IBC with a rigid plastics inner receptacle encased in a rigid reconstituted wood outer casing, for solids filled or discharged by gravity	E
16	11HG1	Composite IBC with a rigid plastics inner receptacle encased in a rigid fibreboard outer casing, for solids filled or discharged by gravity	E
17	11HL1	Composite IBC with a rigid plastics inner receptacle encased in a rigid textile outer casing, for solids filled or discharged by gravity	E
18	11HM1	Composite IBC with a rigid plastics inner receptacle encased in a rigid paper outer casing, for solids filled or discharged by gravity	E
19	11HN1	Composite IBC with a rigid plastics inner receptacle encased in a rigid metal (other than steel or aluminium) outer casing, for solids filled or discharged by gravity	E
50	11HA2	Composite IBC with a flexible plastics inner receptacle encased in a rigid steel outer casing, for solids filled or discharged by gravity	E
51	11HH2	Composite IBC with a flexible plastics inner receptacle encased in a rigid plastics outer casing, for solids filled or discharged by gravity	E
52	11HB2	Composite IBC with a flexible plastics inner receptacle encased in a rigid aluminium outer casing, for solids filled or discharged by gravity	E
53	11HC2	Composite IBC with a flexible plastics inner receptacle encased in a rigid natural wood outer casing, for solids filled or discharged by gravity	E
54	11HD2	Composite IBC with a flexible plastics inner receptacle encased in a rigid plywood outer casing, for solids filled or discharged by gravity	E
55	11HF2	Composite IBC with a flexible plastics inner receptacle encased in a rigid reconstituted wood outer casing, for solids filled or discharged by gravity	E
56	11HG2	Composite IBC with a flexible plastics inner receptacle encased in a rigid fibreboard outer casing, for solids filled or discharged by gravity	E
57	11HL2	Composite IBC with a flexible plastics inner receptacle encased in a rigid textile outer casing, for solids filled or discharged by gravity	E
58	11HM2	Composite IBC with a flexible plastics inner receptacle encased in a rigid paper outer casing, for solids filled or discharged by gravity	E
59	11HN2	Composite IBC with a flexible plastics inner receptacle encased in a rigid metal (other than steel or aluminium) outer casing, for solids filled or discharged by gravity	E
60	13H1	Flexible IBC made of woven plastics without coating or liner, for solids, filled or discharged by gravity	E
61	13H2	Flexible IBC made of woven plastics, coated, for solids, filled or discharged by gravity	E
62	13H3	Flexible IBC made of woven plastics with liner, for solids, filled or discharged by gravity	E
63	13H4	Flexible IBC made of woven plastics, coated and with liner, for solids, filled or discharged by gravity	E
64	13H5	Flexible IBC made of plastics film, for solids, filled or discharged by gravity	E
65	13L1	Flexible IBC made of textile without coating or liner, for solids, filled or discharged by gravity	E
66	13L2	Flexible IBC made of textile, coated, for solids, filled or discharged by gravity	E
67	13L3	Flexible IBC made of textile, with liner, for solids, filled or discharged by gravity	E
68	13L4	Flexible IBC made of textile, coated and with liner, for solids, filled or discharged by gravity	E
69	13M1	Flexible IBC made of paper, multiwall, for solids, filled or discharged by gravity	E
70	13M2	Flexible IBC made of paper, multiwall, water resistant, for solids, filled or discharged by gravity	E
71	21A	Rigid steel IBC for solids, filled or discharged under pressure	E
72	21B	Rigid aluminium IBC for solids, filled or discharged under pressure	E
73	21N	Rigid metal (other than steel or aluminium) IBC for solids, filled or discharged under pressure	E
74	21H1	Rigid plastics IBC for solids, filled or discharged under pressure, fitted with structural equipment	E
75	21H2	Rigid plastics IBC for solids, filled or discharged under pressure, freestanding	E
76	21HA1	Composite IBC with a rigid plastics inner receptacle encased in a rigid steel outer casing, for solids filled or discharged under pressure	E
77	21HH1	Composite IBC with a rigid plastics inner receptacle encased in a rigid plastics outer casing, for solids filled or discharged under pressure	E
78	21HB1	Composite IBC with a rigid plastics inner receptacle encased in a rigid aluminium outer casing, for solids filled or discharged under pressure	E
79	21HC1	Composite IBC with a rigid plastics inner receptacle encased in a rigid natural wood outer casing, for solids filled or discharged under pressure	E
80	21HD1	Composite IBC with a rigid plastics inner receptacle encased in a rigid plywood outer casing, for solids filled or discharged under pressure	E
81	21HF1	Composite IBC with a rigid plastics inner receptacle encased in a rigid reconstituted wood outer casing, for solids filled or discharged under pressure	E
82	21HG1	Composite IBC with a rigid plastics inner receptacle encased in a rigid fibreboard outer casing, for solids filled or discharged under pressure	E
83	21HL1	Composite IBC with a rigid plastics inner receptacle encased in a rigid textile outer casing, for solids filled or discharged under pressure	E
84	21HM1	Composite IBC with a rigid plastics inner receptacle encased in a rigid paper outer casing, for solids filled or discharged under pressure	E
85	21HN1	Composite IBC with a rigid plastics inner receptacle encased in a rigid metal (other than steel or aluminium) outer casing, for solids filled or discharged under pressure	E
86	21HA2	Composite IBC with a flexible plastics inner receptacle encased in a rigid steel outer casing, for solids filled or discharged under pressure	E
87	21HH2	Composite IBC with a flexible plastics inner receptacle encased in a rigid plastics outer casing, for solids filled or discharged under pressure	E
88	21HB2	Composite IBC with a flexible plastics inner receptacle encased in a rigid aluminium outer casing, for solids filled or discharged under pressure	E
89	21HC2	Composite IBC with a flexible plastics inner receptacle encased in a rigid natural wood outer casing, for solids filled or discharged under pressure	E
90	21HD2	Composite IBC with a flexible plastics inner receptacle encased in a rigid plywood outer casing, for solids filled or discharged under pressure	E
91	21HF2	Composite IBC with a flexible plastics inner receptacle encased in a rigid reconstituted wood outer casing, for solids filled or discharged under pressure	E
92	21HG2	Composite IBC with a flexible plastics inner receptacle encased in a rigid fibreboard outer casing, for solids filled or discharged under pressure	E
93	21HL2	Composite IBC with a flexible plastics inner receptacle encased in a rigid textile outer casing, for solids filled or discharged under pressure	E
94	21HM2	Composite IBC with a flexible plastics inner receptacle encased in a rigid paper outer casing, for solids filled or discharged under pressure	E
95	21HN2	Composite IBC with a flexible plastics inner receptacle encased in a rigid metal (other than steel or aluminium) outer casing, for solids filled or discharged under pressure	E
96	31A	Rigid steel IBC for liquids	E
97	31B	Rigid aluminium IBC for liquids	E
98	31N	Rigid metal (other than steel or aluminium) IBC for liquids	E
99	31H1	Rigid plastics IBC for liquids, fitted with structural equipment	E
100	31H2	Rigid plastics IBC for liquids, freestanding	E
101	31HA1	Composite IBC with a rigid plastics inner receptacle encased in a rigid steel outer casing, for liquids	E
102	31HH1	Composite IBC with a rigid plastics inner receptacle encased in a rigid plastics outer casing, for liquids	E
103	31HB1	Composite IBC with a rigid plastics inner receptacle encased in a rigid aluminium outer casing, for liquids	E
104	31HC1	Composite IBC with a rigid plastics inner receptacle encased in a rigid natural wood outer casing, for liquids	E
105	31HD1	Composite IBC with a rigid plastics inner receptacle encased in a rigid plywood outer casing, for liquids	E
106	31HF1	Composite IBC with a rigid plastics inner receptacle encased in a rigid reconstituted wood outer casing, for liquids	E
107	31HG1	Composite IBC with a rigid plastics inner receptacle encased in a rigid fibreboard outer casing, for liquids	E
108	31HL1	Composite IBC with a rigid plastics inner receptacle encased in a rigid textile outer casing, for liquids	E
109	31HM1	Composite IBC with a rigid plastics inner receptacle encased in a rigid paper outer casing, for liquids	E
110	31HN1	Composite IBC with a rigid plastics inner receptacle encased in a rigid metal (other than steel or aluminium) outer casing, for liquids	E
137	31HA2	Composite IBC with a flexible plastics inner receptacle encased in a rigid steel outer casing, for liquids	E
138	31HH2	Composite IBC with a flexible plastics inner receptacle encased in a rigid plastics outer casing, for liquids	E
139	31HB2	Composite IBC with a flexible plastics inner receptacle encased in a rigid aluminium outer casing, for liquids	E
140	31HC2	Composite IBC with a flexible plastics inner receptacle encased in a rigid natural wood outer casing, for liquids	E
141	31HD2	Composite IBC with a flexible plastics inner receptacle encased in a rigid plywood outer casing, for liquids	E
142	31HF2	Composite IBC with a flexible plastics inner receptacle encased in a rigid reconstituted wood outer casing, for liquids	E
143	31HG2	Composite IBC with a flexible plastics inner receptacle encased in a rigid fibreboard outer casing, for liquids	E
144	31HL2	Composite IBC with a flexible plastics inner receptacle encased in a rigid textile outer casing, for liquids	E
145	31HM2	Composite IBC with a flexible plastics inner receptacle encased in a rigid paper outer casing, for liquids	E
146	31HN2	Composite IBC with a flexible plastics inner receptacle encased in a rigid metal (other than steel or aluminium) outer casing, for liquids	E
