See remark 1) to the table in 2.5.3.2.4:
"Diluent type B may always be replaced by diluent type A. The boiling point of diluent type B shall be at least 60°C higher than the SADT of the organic peroxide."

Note: This remark applies only to the carriage of organic peroxides in packagings.