Permitted only if the substance to be transported cannot become liquid during transport.

Special packing provision B4:
Flexible, fibreboard or wooden IBCs shall be sift-proof and water-resistant or shall be fitted with a sift-proof and water-resistant liner.