Combination packagings are authorized.

The general provisions of 4.1.1 and 4.1.3 shall be met.

Additional provisions:
1. Packagings shall have a minimum ullage of 10%.
2. Packagings shall be vented.