T50

This portable tank instruction applies to non-refrigerated liquefied gases and chemicals under pressure (UN Nos. 3500, 3501, 3502, 3503, 3504 and 3505). 

The general provisions of 4.2.2 and the provisions of 6.7.3 shall be met.  

Footnote a) to Maximum allowable working pressure (bar):
(See definition of "Design reference temperature" in 6.7.3.1).


Note concerning Pressure relief provisions:
The word "Normal" in the pressure relief column indicates that a frangible disc as specified in 6.7.3.7.3 is not required.
