The following packagings are authorized, provided that the general provisions of 4.1.1 and 4.1.3 are met:

|    Combination packagings    |   Inner packagings    |  Outer packagings  |
|                              |   maximum capacity    |  maximum net mass  |
+------------------------------+-----------------------+--------------------+
| Boxes (4A, 4B, 4N, 4C1, 4C2, |          5 l          |        125 kg      |
| 4D, 4H2) or drums (1A1, 1A2, |                       |                    |
| 1B1, 1B2, 1N1, 1N2, 1H1, 1H2,|                       |                    |
| 1D) or jerricans (3A1, 3A2,  |                       |                    |
| 3B1, 3B2, 3H1, 3H2) with     |                       |                    |
| glass, plastics or metal     |                       |                    |
| inner packagings             |                       |                    |
|                              |                       |                    |
| Fibreboard box (4G) or fibre |          2 l          |         50 kg      |
| drum (1G), with plastics or  |                       |                    |
| metal inner packagings each  |                       |                    |
| in a plastics bag            |                       |                    |
+------------------------------+-----------------------+--------------------+

Additional provisions:
1 Packagings shall have a minimum ullage of 10%.
2 Packagings shall be vented.