According to the IMSBC Code, the substance is dangerous when transported in bulk (Class MHB) and has the following hazardous properties:
CB: combustible solid and/or
SH: self-heating solid and/or
CR: corrosive solid