According to special provision 238, .2, non-spillable batteries are not subject to the provisions of the IMDG Code if, at a temperature of 55 °C, the electrolyte will not flow from a ruptured or cracked case and there is no free liquid to flow and if, as packaged for transport, the terminals are protected from short circuit.