Note:
This substance shall meet the provisions of sections 2.3.2.2 and 2.3.2.5 for classification as packing group III. The capacity of the receptacles used shall not exceed 450 l. Otherwise, or when transported in larger quantities (more than 450 liters), the provisoions of packing group II apply.

The general provisions of 4.1.1, 4.1.2 and 4.1.3 shall be met.