According to the IMSBC Code, the substance is dangerous when transported in bulk (Class MHB) and has the following hazardous properties:
SH: self-heating solid and/or
CR: corrosive solid and/or
TX: toxic solid