According to the IMSBC Code, the substance is dangerous when transported in bulk (Class MHB) and has the following hazardous properties:
WF: solid that evolve flammable gas when wet and/or
WT: solid that evolve toxic gas when wet and/or
TX: toxic solid