The following combination packagings are authorized provided that the general provisions of 4.1.1 and 4.1.3 are met:

|      Inner packagings      |      Outer packagings       |  Maximum capacity/ |
|                            |                             |  maximum net mass  |
+----------------------------+-----------------------------+--------------------+
|   Glass 5 L                |  Boxes                      |       125 kg       |
|   Plastics 5 L             |     aluminium (4B)          |       125 kg       |
|   Metal 5 L                |     natural wood, ordinary  |       125 kg       |
|                            |                       (4C1) |                    |
|                            |     natural wood, sift-proof|       125 kg       |
|                            |        walls (4C2)          |                    |
|                            |     plywood (4D)            |       125 kg       |
|                            |     fibreboard (4G)         |       125 kg       |
|                            |     plastics, solid (4H2)   |       125 kg       |
|                            |  Drums                      |                    |
|                            |     aluminium, removable    |       125 kg       |
|                            |        head (1B2)           |       125 kg       |
|                            |     fibre (1G)              |       125 kg       |
|                            |     other metal, removable  |       125 kg       |
|                            |        head (1N2)           |       125 kg       |
|                            |     plastics, removable head|       125 kg       |
|                            |                  (1H2)      |       125 kg       |
|                            |     plywood (1D)            |       125 kg       |
|                            |  Jerricans                  |                    |
|                            |     aluminium, removable    |       125 kg       |
|                            |         head (3B2)          |                    |
|                            |     plastics, removable head|       125 kg       |
|                            |         head (3H2)          |                    |
+----------------------------+-----------------------------+--------------------+