Because this BAM number assumes that the substance is liable to become liquid during transport, it shall not be transported in IBCs under these circumstances (see 4.1.3.4 of the IMDG Code).

When the substance does not become liquid during transport, the transport in IBC is permitted (see the relevant BAM number with the suffix "solid").