This substance is listed in tank instruction T23 in 4.2.5.2.6 of the IMDG Code. Since 1 January 2019, the substances listed in tank instruction T23 may also be carried packed in accordance with packing method OP8 of packing instruction P520 of 4.1.4.1, with the same control and emergency temperatures, if applicable.

The carriage of peroxyacetic acid, Type F in packagings is also possible under UN No. 3109 under BAM Nos. 6716 and 9023.

See footnote § in 4.2.5.2.6, Tank instruction T23:
Formulation derived from distillation of peroxyacetic acid originating from peroxyacetic acid in concentration of not more than 41% with water, total active oxygen (peroxyacetic acid + H2O2) <= 9.5%, which fulfils the criteria of 2.5.3.3.2.6. "CORROSIVE" subsidiary hazard placard required (Model No. 8, see 5.2.2.2.2).