Combination packagings are authorized.

The general provisions of 4.1.1 and 4.1.3 shall be met.

Special packing provision PP10:
For UN 1791, for packing group II, and UN Nos. 2014 and 3149, the packaging shall be vented.