The maximum degree of filling (in %) for solids transported above their melting points and for elevated temperature liquids shall be determined by the following formula in accordance with 4.2.1.9.5.1:

Degree of filling = 95 (dr/df)

where
df =  density of the liquid at the mean temperature of the liquid during filling
dr = density of the liquid at the maximum mean bulk temperature during transport