See remarks 13), 16) and 19) on the table in 2.5.3.2.4:

13) "CORROSIVE" subsidiary hazard label required (Model No.8, see 5.2.2.2.2).

16) Peroxyacetic acid formulations which fulfil the criteria of 2.5.3.3.2.6.

19) Mixtures with hydrogen peroxide, water and acid(s).