The provisions of the individual schedule in the IMSBC Code do not apply to Aluminium smelting by-products or Aluminium remelting by-products (UN 3170).
The substance classified as MHB has the following hazardous properties:
WF: solid that evolve flammable gas when wet and/or
WT: solid that evolve toxic gas when wet and/or
CR: corrosive solid