Combination packagings are authorized.

The general provisions of 4.1.1 and 4.1.3 shall be met.

Special packing provision PP5:
For UN 1204, packagings shall be so constructed that explosion is not possible by reason of increased internal pressure. Gas cylinders and gas receptacles shall not be used for these substances.