The following packagings are authorized, provided that the general provisions of 4.1.1 and 4.1.3 are met:

Drums (1A2, 1B2, 1N2, 1H2, 1D, 1G);
Boxes (4A, 4B, 4N, 4C1, 4C2, 4D, 4F, 4G, 4H1, 4H2);
Jerricans (3A2, 3B2, 3H2).

Packagings shall conform to the packing group II performance level.

The generator(s) shall be transported in a package which meets the following requirements when one generator in the package is actuated:

(1) Other generators in the package will not be actuated;
(2) Packaging material will not ignite; and
(3) The outside surface temperature of the completed package shall not exceed 100°C.