Fumigation warning mark
* Insert details as appropriate
The fumigation warning mark shall be rectangular and shall not be less than 400 mm wide and 300 mm high. The minimum width of the outer line shall be 2 mm. The mark shall be in black print on a white background with lettering not less than 25 mm high.