See remarks 3) and 13) on the table in 2.5.3.2.4:

3) "EXPLOSIVE" subsidiary hazard label required. (Model No. 1, see 5.2.2.2.2).

13) "CORROSIVE" subsidiary hazard label required (Model No. 8, see 5.2.2.2.2).