For UN Nos. 0074, 0113, 0114, 0129, 0130, 0135 and 0224, the following conditions shall be met:

.1 inner packagings shall not contain more than 50 g of explosive substance (quantity corresponding to dry substance);
.2 compartments between dividing partitions shall not contain more than one inner packaging, firmly fitted; and
.3 the outer packaging may be partitioned into up to 25 compartments.