Packagings: see topic "Combination packagings"

Vehicles with an individual net mass of 30 kg or more:

(a) may be loaded into crates or secured to pallets;

(b) may be transported unpackaged providing that the vehicle is capable of remaining upright during Transport without additional support and the vehicle provides adequate protection to the battery so that no damage to the battery can occur; or

(c) where the vehicles have the potential to topple over during transport (e.g. motor cycles), may be transported unpackaged in a cargo transport unit fitted out with the means to prevent toppling in transport, such as by the use of bracing, frames or racking.