The following packagings are authorized provided the general provisions of 4.1.1 and 4.1.3 are met:

|  Combination packagings                               |   Maximum net mass  |
+-------------------------------------------------------+---------------------+
| (1) Outer packagings:                                 |         75 kg       |
|     (1A1, 1A2, 1B1, 1B2, 1N1, 1N2, 1H1, 1H2, 1D, 1G,  |                     |
|     4A, 4B, 4N, 4C1, 4C2, 4D, 4F, 4G, 4H2)            |                     |
|     Inner packagings:                                 |                     |
|     Glass receptacles with a maximum capacity of 5 L  |                     |
| (2) Outer packagings:                                 |         75 kg       |
|     (1A1, 1A2, 1B1, 1B2, 1N1, 1N2, 1H1, 1H2, 1D, 1G,  |                     |
|     4A, 4B, 4N, 4C1, 4C2, 4D, 4F, 4G, 4H2)            |                     |
|     Inner packagings:                                 |                     |
|     Glass receptacles with a maximum capacity of 30 L |                     |
| (3) Outer packagings:                                 |        125 kg       |
|     (1G, 4F or 4G)                                    |                     |
|     Inner packagings:                                 |                     |
|     Metal receptacles with a maximum capacity of 40 L |                     |
| (4) Outer packagings:                                 |        225 kg       |
|     (1A1, 1A2, 1B1, 1B2, 1N1, 1N2, 1H1, 1H2, 1D, 4A,  |                     |
|     4B, 4N, 4C1 ,4C2, 4D, 4F, 4G, 4H2)                |                     |
|     Inner packagings:                                 |                     |
|     Metal receptacles with a maximum capacity of 40 L |                     |
+-------------------------------------------------------+---------------------+