For transportation under the IMSBC Code:
The individual schedule of the IMSBC Code applies only to cargoes that would fall into packing group III under the IMDG Code when transported in packaged form.
The substance additionally classified as MHB has the following hazardous properties:
WT: solid that evolve toxic gas when wet and/or
CR: corrosive solid and/or
TX: toxic solid