To prevent the tank bursting in any event, including fire engulfment, it shall be provided with pressure relief devices which are adequate in relation to the capacity of the tank and to the nature of the substance transported. The device shall also be compatible with the substance.