(1) Packaged articles:

The general provisions of 4.1.1 and 4.1.3 shall be met.

The rigid large packagings shall met the packing group III performance level.

The packagings shall be designed and constructed to prevent movement of the articles and inadvertent operation during normal conditions of transport.

(2) Unpackaged articles:

The articles may also be transported unpackaged in dedicated handling devices, vehicles, containers or wagons when moved to, from, or between where they are manufactured and an assembly plant including intermediate handling locations.

Additional provision:
 
Any pressure receptacle shall be in accordance with the requirements of the competent authority for the substance(s) contained in the pressure receptacle(s).