The degree of filling prescribed in 4.2.1.9.2 shall not be exceeded:

Degree of filling = 97 / (1 + alpha x (tr - tf))

where
alpha = mean coefficient of cubical expansion of the liquid between tf and tr;
tr = maximum mean bulk temperature during carriage [°C];
tf = mean temperature of the liquid during filling [°C].