The following packagings are authorized provided the general provisions of 4.1.1 and 4.1.3 are met:

|  Inner packagings   |    Outer packagings    |   Code   | Maximum * |
+---------------------+------------------------+----------+-----------+
| Glas          10 kg | Drums                  |          |           |
| Plastics 1)   30 kg |     steel              | 1A1, 1A2 |   400 kg  |
| Metal         40 kg |     aluminium          | 1B1, 1B2 |   400 kg  |
| Paper 1),2)   10 kg |     other metal        | 1N1, 1N2 |   400 kg  |
| Fibre 1),2)   10 kg |     plastics           | 1H1, 1H2 |   400 kg  |
|                     |     plywood            | 1D       |   400 kg  |
|                     |     fibre 1)           | 1G       |   400 kg  |
|                     +------------------------+----------+-----------+
|                     | Boxes                  |          |           |
|                     |     steel              | 4A       |   400 kg  |
|                     |     aluminium          | 4B       |   400 kg  |
|                     |     other metal        | 4N       |   400 kg  |
|                     |     natural wood       | 4C1      |   400 kg  |
|                     |     natural wood with  | 4C2      |   400 kg  |
|                     |       sift-proof walls |          |           |
|                     |     plywood            | 4D       |   400 kg  |
|                     |     reconstituted wood | 4F       |   400 kg  |
|                     |     fibreboard 1)      | 4G       |   400 kg  |
|                     |     expanded plastics  | 4H1      |    60 kg  |
|                     |     solid plastics     | 4H2      |   400 kg  |
|                     +------------------------+----------+-----------+
|                     | Jerricans              |          |           |
|                     |     steel              | 3A1, 3A2 |   120 kg  |
|                     |     aluminium          | 3B1, 3B2 |   120 kg  |
|                     |     plastics           | 3H1, 3H2 |   120 kg  |
+---------------------+------------------------+----------+-----------+

* Maximum net mass

1) These packagings shall be sift-proof.
2) These inner packagings shall not be used when the substances being transported may become liquid during transport.