The following packagings are authorized provided the general provisions of 4.1.1 and 4.1.3 are met:

|  Inner packagings 1)|    Outer packagings    |   Code   | Maximum * |
+---------------------+------------------------+----------+-----------+
| Glas           2 kg | Drums                  |          |           |
| Plastic       15 kg |     steel              | 1A1, 1A2 |   400 kg  |
| Metal         20 kg |     aluminium          | 1B1, 1B2 |   400 kg  |
|                     |     other metal        | 1N1, 1N2 |   400 kg  |
|                     |     plastics           | 1H1, 1H2 |   400 kg  |
|                     |     plywood            | 1D       |   400 kg  |
|                     |     fibre              | 1G       |   400 kg  |
|                     +------------------------+----------+-----------+
|                     | Boxes                  |          |           |
|                     |     steel              | 4A       |   400 kg  |
|                     |     aluminium          | 4B       |   400 kg  |
|                     |     other metal        | 4N       |   400 kg  |
|                     |     natural wood       | 4C1      |   250 kg  |
|                     |     natural wood with  | 4C2      |   250 kg  |
|                     |       sift-proof walls |          |           |
|                     |     plywood            | 4D       |   250 kg  |
|                     |     reconstituted wood | 4F       |   125 kg  |
|                     |     fibreboard         | 4G       |   125 kg  |
|                     |     expanded plastics  | 4H1      |    60 kg  |
|                     |     solid plastics     | 4H2      |   250 kg  |
|                     +------------------------+----------+-----------+
|                     | Jerricans              |          |           |
|                     |     steel              | 3A1, 3A2 |   120 kg  |
|                     |     aluminium          | 3B1, 3B2 |   120 kg  |
|                     |     plastics           | 3H1, 3H2 |   120 kg  |
+---------------------+------------------------+----------+-----------+

* Maximum net mass

1) Inner packagings shall be hermetically sealed (e.g. by taping or by threaded closures).