The following packagings are authorized, provided that the general provisions of 4.1.1 and 4.1.3 are met:

Outer packagings:
Drums (1A1, 1A2, 1B1, 1B2, 1N1, 1N2, 1H1, 1H2, 1D, 1G);
Boxes (4A, 4B, 4N, 4C1, 4C2, 4D, 4F, 4G, 4H1, 4H2);
Jerricans (3A1, 3A2, 3B1, 3B2, 3H1, 3H2).

Inner packagings:
Matches shall be tightly packed in securely closed inner packagings to prevent accidental ignition under normal conditions of transport.

The maximum gross mass of the package shall not exceed 45 kg except for fibreboard boxes which shall not exceed
30 kg.

Packagings shall conform to the packing group III performance level.