An oxygen generator, chemical, containing oxidizing substances shall meet the following conditions:

.1 the generator, when containing an explosive device, shall only be transported under this entry when excluded from class 1 in accordance with 2.1.3 of this Code;

.2 the generator, without its packaging, shall be capable of withstanding a 1.8 m drop test onto a rigid, non-resilient, flat and horizontal surface, in the position most likely to cause damage, without loss of its contents and without actuation; and

.3 when the generator is equipped with an actuating device, it shall have at least two positive means of preventing unintentional actuation.