Neutron radiation detectors containing non-pressurized boron trifluoride gas may be transported under this entry provided that the following conditions are met:

.1 Each radiation detector shall meet the following conditions:

	.1	the pressure in each detector shall not exceed 105 kPa absolute at 20°C;

	.2	the amount of gas shall not exceed 13 g per detector;

	.3	each detector shall be manufactured under a registered quality assurance programme;

Note: The application of ISO 9001:2008 may be considered acceptable for this purpose.

	.4	each neutron radiation detector shall be of welded metal construction with brazed metal
		to ceramic feed through assemblies. These detectors shall have a minimum burst pressure
		of 1800 kPa as demonstrated by design type qualification testing; and

	.5	each detector shall be tested to a 1 x 10-10 cm³/s leak tightness standard before
		filling.

.2 Radiation detectors transported as individual components shall be transported as follows:

	.1	detectors shall be packed in a sealed intermediate plastics liner with sufficient absorbent 
        or adsorbent material to absorb or adsorb the entire gas contents;

	.2	they shall be packed in strong outer packaging. The completed package shall be capable
		of withstanding a 1.8 m drop test without leakage of gas contents from detectors;

	.3	the total amount of gas from all detectors per outer packaging shall not exceed 52 g.

.3 Completed neutron radiation detection systems containing detectors meeting the conditions of .1 shall be transported as follows:

	.1	the detectors shall be contained in a strong sealed outer casing;

	.2	the casing shall contain sufficient absorbent or adsorbent material to absorb or adsorb the entire 
		gas contents; and

	.3	the completed systems shall be packed in strong outer packagings capable of
		withstanding a 1.8 m drop test without leakage unless a system's outer casing affords
		equivalent protection.

Packing instruction P200 of 4.1.4.1 is not applicable.

The transport document shall include the statement "Transport in accordance with special provision 373".

Neutron radiation detectors containing not more than 1 g of boron trifluoride, including those with solder glass joints, are not subject to this Code  provided they meet the requirements in paragraph .1 and are packed in accordance with paragraph .2. Radiation detection systems containing such detectors are not subject to this Code provided they are packed in accordance with paragraph .3.

Neutron radiation detectors shall be stowed in accordance with stowage Category A.