Special packing provision B 4:
Flexible, fibreboard or wooden IBCs shall be sift-proof and water-resistant or shall be fitted with a sift-proof and water-resistant liner.

Authorized only when the substance being carried may not become liquid during carriage.