The following packagings are authorized, provided that the general provisions of 4.1.1 and 4.1.3 are met:

| Combination packagings                               | Maximum * |
+------------------------------------------------------+-----------+
| (1) Glass receptacles with a maximum capacity of     |   75 kg   |
| 5 litres in 1A1, 1A2, 1B1, 1B2, 1N1, 1N2, 1H1, 1B2,  |           |
| 1N1, 1N2, 1H1, 1H2, 1D, 1G, 4A, 4B, 4N, 4C1, 4C2,    |           |
| 4D, 4F, 4G or 4H2 outer packagings.                  |           |
|                                                      |           |
| (2) Plastics receptacles with a maximum capacity of  |   75 kg   |
| 30 litres in 1A1, 1A2, 1B1, 1B2, 1N1, 1N2, 1H1, 1H2, |           |
| 1D, 1G, 4A, 4B, 4N, 4C1, 4C2, 4D, 4F, 4G or 4H2      |           |
| outer packagings.                                    |           |
|                                                      |           |
| (3) Metal receptacles with a maximum capacity of     |  125 kg   |
| 40 litres in 1G, 4F or 4G outer packagings           |           |
|                                                      |           |
| (4) Metal receptacles with a maximum capacity of     |  225 kg   |
| 40 litres in 1A1, 1A2, 1B1, 1B2, 1N1, 1N2, 1H1, 1H2, |           |
| 1D, 4A, 4B, 4N, 4C1, 4C2, 4D oder 4H2 outer          |           |
| packagings.                                          |           |
+------------------------------------------------------+-----------+