(1) Packaged articles:

The general provisions of 4.1.1 and 4.1.3 shall be met.

The large packagings shall conform to the packing group III performance level.

The packagings shall be designed and constructed to prevent movement of the articles and inadvertent operation during normal conditions of carriage.

(2) Unpackaged articles:

The articles may also be carried unpackaged in dedicated handling devices or cargo transport units when moved to, from, or between where they are manufactured and an assembly plant including intermediate handling locations.


Additional requirement
Any pressure receptacle shall be in accordance with the requirements of the competent authority for the substance(s) contained in the pressure receptacle(s).