Packagings: see topic "Combination packagings"

Unpackaged articles:

Except for UN 3559, the articles may also be carried unpackaged in dedicated handling devices or cargo transport units when moved to, from, or between where they are manufactured and an assembly plant including intermediate handling locations.


Additional requirement
Any pressure receptacle shall be in accordance with the requirements of the competent authority for the substance(s) contained therein.