Special packing provision PP 92:
For UN No. 3531, packagings shall be designed and constructed to permit the release of gas or vapour to pre-vent a build-up of pressure that could rupture the packagings in the event of loss of stabilization.