The periodic inspections according to 6.8.2.4.2 shall be performed
- tank-wagons, demountable tanks and battery wagons: no later than every four years;
- tank-containers, tank swap bodies and MEGCs: no later than every two and a half years.