The design type shall be tested and marked appropriately.

Note:
In the opinion of BAM, design types 0A1 and 0A2 light-gauge metal packagings are not suitable for substances with a vapour pressure of more than 110 kPa at 50 °C. We do not recommend using these packagings for this substance, although packing instruction R001 is listed in Table A of RID. The joint meeting has been informed.