Special packing provision PP 84:
For UN No. 1057, rigid outer packagings meeting the packing group II performance level shall be used. The packagings shall be designed and constructed and arranged to prevent movement, inadvertent ignition of the devices or inadvertent release of flammable gas or liquid.

NOTE: For waste lighters collected separately see Chapter 3.3, special provision 654.


Special packing provision RR 5 specific to RID:
Notwithstanding special packing provision PP 84, only the general provisions of 4.1.1.1, 4.1.1.2 and 4.1.1.5 to 4.1.1.7 need be complied with if the gross mass of the package is not more than 10 kg.

NOTE: For waste lighters collected separately see Chapter 3.3, special provision 654.