Battery mark:
Note: This mark is necessary for the transport of lithium cells or batteries or sodium ion cells or batteries according to special provision 188 or 400. In this case a label model No. 9A is not required.
The mark shall be in the form of a rectangle or a square with hatched edging. The dimensions shall be a minimum of 100 mm wide x 100 mm high and the minimum width of the hatching shall be 5 mm. The symbol (group of batteries, one damaged and emitting flame, above the UN numbers) shall be black on white or suitable contrasting background. The hatching shall be red. If the size of the package so requires, the dimensions/line thickness may be reduced to not less than 100 mm wide x 70 mm high. Where dimensions are not specified, all features shall be in approximate proportion to those shown.

* Place for UN number(s)

Note: see Transitional measure 1.6.1.49

The mark shown in Figure 5.2.1.9.2 applicable until 31 December 2022, may continue to be applied until 31 December 2026.