Combination packagings are authorized.
The general provisions of 4.1.1 and 4.1.3 shall be met.

Additional requirements
1. Packagings shall have a maximum filling degree of 90%.
2. Packagings shall be vented.