Combination packagings are authorized.
The general provisions of 4.1.1 and 4.1.3 shall be met.

Special packing provision PP 5:
For UN No. 1204, packagings shall be so constructed that explosion is not possible by reason of increased internal pressure. Cylinders, tubes and pressure drums shall not be used for these substances.