Tank-wagons, demountable tanks and battery-wagons:
The hydraulic pressure tests shall be performed no later than every 4 years.

Tank-containers, tank swap bodies and MEGCs:
The hydraulic pressure tests shall be performed no later than every 2,5 years.