Shunting label conforming Model 15
Loose shunting or hump shunting forbidden. Shall be accompanied by a motive power unit. Shall not bump, or be bumped by, other wagons.
Three triangles, red, with black exclamation mark 
Width: minimum 105 mm
Hight: minimum 74 mm